# Description:

* Bunker doors interior with electromechanical drive, sliding, with shielding thickness:

DOOR TrueBeam

Shielding: **Pb 50 mm, BPE 100 mm**

Dimensions of the concrete opening: w 1 450 mm, h 2 100 mm

Dimensions of the door leaf: w 1 750 mm, h 2 200 mm

Dimensions of the door leaf overlaps the concrete opening by cca. 150mm (at each side) and 100 mm on the top.

* Bunker doors interior with electromechanical drive, sliding, with shielding thickness:

DOOR Halcyon

Shielding: **Pb 7 mm**

Dimensions of the concrete opening: w 1 450 mm, h 2 100 mm

Dimensions of the door leaf: w 1 750 mm, h 2 200 mm

Dimensions of the door leaf overlaps the concrete opening by cca. 150mm (at each side) and 100 mm on the top.