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LLC Gardabani Sewage Treatment Plant (GST) announces an electronic tender on procurement of the Dewatered Sludge Hooklift Containers, Hooklift System and Tractor.


























1. PURCHASER
LLC Gardabani Sewage Treatment Plant (GST) (Registration number: 203828313; Registration Country: Georgia)


2. Scope of Supply

The Supplier shall provide a complete, operational and mutually compatible system consisting of:
· Two (2) dewatered sludge Hooklift-compatible containers, nominal capacity 20 m³ each;
· One (1) Hooklift system, fully compatible with the supplied containers;
· One (1) tractor, suitable for transporting and operating the supplied Hooklift system.

The Supplier shall be responsible for ensuring compatibility between the tractor, Hooklift system and containers.
The scope of supply shall include all standard components, accessories, fittings, equipment and documentation
necessary for safe and normal operation of the complete system.

3. Technical Requirements
The technical requirements and parameters are provided in Annex No. 2. Please refer to the Annex and review it
carefully.


4. Commercial, Technical and Price table
Annex No. 3 contains the Commercial, Technical and Financial Offer Form to be completed by the Bidder.


5. Documentation to be Supplied
The Supplier shall provide, at minimum:
· Manufacturer’s technical datasheet;
· Operating manual;
· Safety instructions;
· Maintenance/service manual;
· Spare parts catalogue;
· Hydraulic system documentation, where applicable;
· Warranty documentation;
· Certificates of conformity/compliance, where applicable;
· Manufacturer’s declaration of conformity, where applicable;
· Recommended maintenance schedule;
· List of recommended consumables and spare parts.
All documentation shall be provided in English unless otherwise agreed with GST.

6. Delivery Requirements

The complete scope of supply shall be delivered during calendar year 2027.
The Bidder shall specify the exact proposed delivery date in its commercial offer.
The proposed delivery date shall apply to the complete scope of supply unless the Bidder explicitly proposes a different
delivery schedule for individual items.
Any proposed partial delivery shall be clearly identified in the Bidder’s offer and shall be subject to GST’s approval.
The Bidder shall specify:
· exact delivery date;
· proposed delivery schedule, if applicable.
The delivery location shall be Gardabani Sewage Treatment Plant, Georgia, unless otherwise specified by GST.
The equipment shall be delivered complete and ready for operation.

7. Payment Terms

Payment for the supplied Goods shall be made during calendar year 2027 in accordance with the payment terms agreed in the contract.
The Bidder shall clearly specify its proposed payment terms in the Commercial Offer.
If the Bidder requires an advance payment, it shall clearly state:
· required advance payment amount;
· If no advance payment is required, the Bidder shall state: “No advance payment required.”

Where an advance payment is requested, GST reserves the right to require an advance payment bank guarantee issued by a bank acceptable to GST.

The amount, validity period and other conditions of such guarantee shall be determined in accordance with the contractual requirements established by GST.

8. Warranty Requirements

The Bidder shall provide a minimum warranty period of: 12 months
The Bidder shall clearly state the proposed warranty period for:
· Containers;
· Hooklift system;
· Tractor.

Where the manufacturer provides a longer warranty period, the longer period shall be stated in the Bidder’s offer.
For the tractor, the Bidder shall also state whether any operating-hour limitation applies to the warranty.
The warranty shall cover manufacturing defects, defects in materials and workmanship under normal operating conditions.

The Bidder shall specify all warranty exclusions.

9. After-Sales Service

The Bidder shall provide after-sales technical support for the supplied equipment.

The Bidder shall specify:
•	availability of service support in Georgia;
•	location of service facilities;
•	service response time;
•	availability of qualified service personnel;
•	availability of spare parts;
•	estimated spare-parts delivery time;
•	preventive maintenance services;
•	warranty repair procedure;
•	technical support contact details.

The Supplier shall ensure reasonable availability of spare parts for the supplied equipment.

The Bidder shall provide information regarding:
· availability of original spare parts;
· estimated spare-parts supply period;
· local stock availability, if any;
· manufacturer’s recommended spare parts;
· consumables required for scheduled maintenance.

The Bidder shall provide a recommended spare-parts list for the first year of operation.

10. Training and Commissioning

The Supplier shall provide basic operational instruction to GST personnel following delivery.
The training shall cover, at minimum:
· safe operation of the tractor;
· Hooklift loading procedure;
· Hooklift unloading procedure;
· container securing;
· safety precautions;
· daily inspection;
· basic maintenance;
· emergency procedures.

The Supplier shall demonstrate the complete system in operating condition after delivery.
The equipment shall be commissioned and demonstrated as a complete compatible system.

NOTE: 
1) All documents and/or information created by the bidder and uploaded in the electronic tender must be signed by an authorized person;
2) All documents and/or information created by the bidder should be confirmed by the electronic signature of the authorized person or the electronic stamp of the company;
11. OTHER REQUIREMENT 

At the time of submission of the proposal, the bidder should not be:
· In the process of bankruptcy;
· In the process of liquidation;
· In a state of temporary suspension of activities.
The Procurer reserves the right to determine the deadline for completion of the tender, change the terms of the tender, notifying the tender participants in a timely manner or terminate the tender at any stage of its progress
The Procurer shall identify the winning supplier to the Tender Committee and notify the decision to all
participating companies. The Purchaser is not obliged to provide the participating company with a verbal or written explanation of any decision related to the competition.
The Purchaser reserves the right to verify any information received from the Bidders, as well as to seek information about the Bidder Company or its activities. If it is proved that the information provided by the bidder is not true or falsified, the bidder will be disqualified.
Please note that the Buyer will not accept any oral questions for further information. 
Questions over the phone will be accepted as an exception.
INFORMATION FOR E-TENDER PARTICIPANTS
1.13.1  Any questions during the tender process must be in writing and the online form of tenders.ge portal must be used;
1.13.2 To participate in the electronic tender, the company must be registered on the website www.tenders.ge
1.13.3 Instructions for participating in the electronic tender on tenders.ge can be found in the attached file:


Contact information:
Procurement representative
Contact person: Giorgi Sotkilava
Address: Georgia, Tbilisi, Mtatsminda district, Medea (Mzia) Jugheli street, №10
Email: gsotkilava@gwp.ge
Tel: +995 322 931111 (4801); 
Mob: +995 577 002761

[bookmark: _Toc454818556]Contact person: Irakli Khvadagadze
Address: Georgia, Tbilisi, Mtatsminda district, Medea (Mzia) Jugheli street, №10
Email: ikhvadagadze@gwp.ge
Tel: +995 322 931111 (1145); +
Mob: 995 599 505067

Contact person: Magda Lomtatidze
Address: Georgia, Tbilisi, Mtatsminda district, Medea (Mzia) Jugheli street, №10
Email: mlomtatidze@gwp.ge
Tel: +995 322 931111 (1145); 
Mob: +995 595 22 66 94
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Technical Requirements

1. Dewatered Sludge Containers

Quantity: 2 (two) units;



Application: The containers shall be specifically suitable for the transportation of dewatered wastewater sludge and shall be suitable for outdoor operation under industrial conditions.



Minimum Technical Requirements

		Parameter

		Minimum Requirement



		Quantity

		2 units



		Nominal capacity

		20 m³ each



		Application

		Dewatered sludge transportation



		Construction

		Heavy-duty welded steel construction



		Operation

		Outdoor / industrial operation



		Corrosion protection

		Corrosion-resistant protective coating



		Hooklift compatibility

		Fully compatible with the supplied Hooklift system



		Loading/unloading

		Suitable for safe mechanical loading and unloading



		Structure

		Reinforced heavy-duty construction



		Unloading

		Rear unloading door



		Support

		Rollers/support rollers suitable for Hooklift operation







The Supplier shall state the actual container capacity, dimensions, tare weight and maximum permissible gross weight in its Technical Compliance Table. The container construction shall be suitable for the weight, characteristics and handling requirements of dewatered sludge. The containers shall be designed to withstand repeated loading, transportation, unloading and outdoor operation. The container shall have appropriate structural reinforcement to ensure safe operation under the intended working conditions. The container shall be equipped with a suitable rear door or equivalent unloading arrangement allowing safe and efficient unloading of the dewatered sludge. The containers shall include all rollers, hook bar/interface components, supports and other standard components necessary for operation with the proposed Hooklift system.



2. Hooklift System

Quantity: 1 (one) unit;



Application: The supplied Hooklift system shall be a heavy-duty system designed for industrial and municipal applications and shall be fully compatible with both supplied 20 m³ containers.

The system shall:

· allow safe loading of the containers;

· allow safe unloading of the containers;

· allow secure transportation of the containers;

· be suitable for repeated industrial use;

· be fully compatible with the proposed tractor;

· be fully compatible with the proposed containers;

· be capable of handling the maximum permissible load of the supplied containers;

· comply with applicable European standards and safety requirements.

The Supplier shall provide the complete Hooklift system, including all components required for normal operation. The Hooklift system shall include all hydraulic, mechanical and structural components required for safe and reliable operation. The system shall have appropriate mechanisms for securing the container during transportation. The Bidder shall clearly describe the method of connecting and operating the Hooklift system with the proposed tractor.

3. Tractor

Quantity: 1 (one) unit;



Application: The tractor shall be suitable for transporting and operating the supplied Hooklift system and shall be capable of safely handling the maximum permissible load of the proposed containers. The tractor shall be suitable for industrial operation at the Gardabani Sewage Treatment Plant and associated transportation activities.



Minimum Technical Requirements

		Parameter

		Minimum / Required Specification



		Quantity

		1 unit



		Engine

		Diesel



		Drive

		4×4



		Engine power

		Minimum 130 hp



		Hydraulic system

		Suitable for supplied Hooklift system



		Hydraulic pump

		Minimum 70 l/min or sufficient for the proposed Hooklift system



		PTO

		Suitable for the supplied Hooklift system



		Transmission

		Suitable for heavy-duty operation and transportation



		Lifting capacity

		Minimum 7,800 kg or sufficient for the proposed Hooklift/container combination



		Application

		Heavy-duty industrial operation



		Air conditioning

		Required



		Air compressor

		Required



		Counterweight

		To be provided as required for safe Hooklift operation







The Bidder may offer a tractor with higher technical specifications than the minimum requirements. The proposed tractor shall be technically compatible with the supplied Hooklift system without requiring modifications that are not included in the Bidder’s offer.

4. Compatibility Requirements

1. The Supplier shall ensure full compatibility between: Tractor → Hooklift System → Containers

2. The Bidder shall confirm that the proposed combination constitutes a complete operational system.

3. Any additional equipment, adapters, hydraulic components, fittings, brackets or other components required for

complete operation shall be included in the offered price.

4. No additional payment shall be accepted for components that are necessary for safe and normal operation of the complete system but were omitted from the initial offer.

5. Safety Requirements

1. All supplied equipment shall be new and suitable for the intended industrial application, unless otherwise explicitly agreed by GST. 

2. The equipment shall comply with applicable European technical and safety requirements. 

3. The Hooklift system shall include appropriate mechanical and/or hydraulic safety locking arrangements to prevent unintended movement or release of the container during transportation. 

4. The Supplier shall provide operating and safety instructions in Georgian and/or English.

6. Corrosion Protection and Finish

The containers shall be suitable for outdoor operation and shall have an appropriate corrosion-resistant protective

coating. The Bidder shall describe:

· steel grade/material;

· surface preparation;

· corrosion protection method;

· primer/coating system;

· final coating;

· coating thickness, where applicable.



7. Condition of Goods

Unless otherwise stated in the Bidder’s offer and expressly accepted by GST:

· all equipment shall be new;

· the tractor shall be a new or unused unit;

· the containers shall be newly manufactured;

· the Hooklift system shall be newly manufactured;

· the supplied equipment shall not have been previously used for commercial or industrial operation.
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Commercial Offer / Price Schedule

The Bidder shall complete the following Commercial Offer:

		№

		Item

		Qty.

		Unit Price EUR

		Total Price EUR



		1

		20 m³ Dewatered Sludge Hooklift Container

		2

		

		



		2

		Hooklift System

		1

		

		



		3

		Tractor suitable for the supplied Hooklift System

		1

		

		



		4

		Standard equipment and accessories

		Included

		

		



		5

		Delivery and transportation to Gardabani -  Wastewater Treatment Plant

		1

		

		



		

		TOTAL PRICE EUR excluding VAT

		

		

		



		

		VAT EUR, if applicable

		

		

		



		

		TOTAL PRICE EUR including VAT

		

		

		







Commercial information to be Provided by the Bidder

		№

		Information

		Bidder’s Offer



		1

		Manufacturer – Containers

		



		2

		Model – Containers

		



		3

		Country of manufacture – Containers

		



		4

		Manufacturer – Hooklift

		



		5

		Model – Hooklift

		



		6

		Country of manufacture – Hooklift

		



		7

		Manufacturer – Tractor

		



		8

		Model – Tractor

		



		9

		Country of manufacture – Tractor

		



		10

		Manufacturing year

		



		11

		Proposed delivery date

		DD/MM/2027



		12

		Delivery location

		Gardabani Wastewater Treatment Plant



		13

		Offer validity period

		



		14

		Payment terms

		___ Days After Delivery



		15

		Advance payment required

		Yes / No



		16

		Advance payment amount

		



		17

		Warranty – Containers

		



		18

		Warranty – Hooklift

		



		19

		Warranty – Tractor

		



		20

		After-sales service location

		



		21

		Service response time

		



		22

		Spare parts availability

		



		23

		Operator training

		Included







Tractor Technical Data

		Parameter

		Bidder’s Offer



		Manufacturer

		



		Model

		



		Country of manufacture

		



		Year of manufacture

		



		Engine power (hp/kW)

		



		Maximum torque (Nm)

		



		Engine displacement

		



		Fuel system

		



		Emission standard

		



		Transmission

		



		Number of forward gears

		



		Number of reverse gears

		



		Wheel formula

		



		Overall length

		



		Overall width

		



		Overall height

		



		Kerb weight

		



		Maximum permissible gross weight

		



		Maximum lifting capacity

		



		Hydraulic pump capacity

		



		Hydraulic operating pressure

		



		Number of hydraulic valves

		



		PTO speeds

		



		Fuel tank capacity

		



		Air conditioning

		Yes/No



		Air compressor

		Yes/No



		Front counterweight

		



		Rear counterweight

		











Hooklift Technical Data

		Parameter

		Bidder to Specify



		Manufacturer

		



		Model

		



		Country of manufacture

		



		Maximum lifting capacity

		



		Maximum container capacity

		



		Suitable container length range

		



		Hook height / hook dimensions

		



		Hydraulic operating pressure

		



		Hydraulic oil flow requirement

		



		Hydraulic cylinder specification

		



		Loading/unloading cycle time

		



		System weight

		



		Required tractor hydraulic capacity

		



		Required PTO characteristics

		



		Safety locking mechanism

		



		Container securing system

		



		Applicable standards

		







Technical Compliance Table

The Bidder shall complete the following table and provide supporting manufacturer documentation where applicable:

		№

		Requirement

		GST Requirement

		Bidder’s Offer

		Comply (Yes/No)

		Supporting Document / Page



		1

		Container quantity

		2 units

		

		

		



		2

		Container capacity

		20 m³ each

		

		

		



		3

		Container application

		Dewatered sludge

		

		

		



		4

		Container construction

		Heavy-duty welded steel

		

		

		



		5

		Corrosion protection

		Required

		

		

		



		6

		Rear unloading door

		Required

		

		

		



		7

		Hooklift compatibility

		Required

		

		

		



		8

		Hooklift system quantity

		1 unit

		

		

		



		9

		Heavy-duty Hooklift

		Required

		

		

		



		10

		Container securing system

		Required

		

		

		



		11

		Tractor quantity

		1 unit

		

		

		



		12

		Engine

		Diesel

		

		

		



		13

		Engine power

		Min. 130 hp

		

		

		



		14

		Drive

		4×4

		

		

		



		15

		Hydraulic capacity

		Min. 70 l/min or sufficient

		

		

		



		16

		Lifting capacity

		Min. 7,800 kg or sufficient

		

		

		



		17

		Air conditioning

		Required

		

		

		



		18

		Air compressor

		Required

		

		

		



		19

		Tractor/Hooklift compatibility

		Required

		

		

		



		20

		Complete system compatibility

		Required

		

		

		



		21

		Operating manuals

		Required

		

		

		



		22

		Spare parts catalogue

		Required

		

		

		



		23

		Warranty

		Min. 12 months

		

		

		



		24

		Delivery

		During 2027

		

		

		



		25

		Exact delivery date

		To be specified

		

		

		







Bidder’s Declaration

The Bidder shall confirm that:

1. The offered equipment complies with the technical requirements specified in this document;

1. The containers, Hooklift system and tractor are fully compatible;

1. The offered system is complete and ready for operation;

1. All necessary standard components are included in the offered price;

1. The proposed equipment is suitable for dewatered sludge transportation;

1. The Bidder has provided accurate technical information;

1. The proposed delivery date falls within calendar year 2027;

1. The Bidder has clearly stated its payment and advance-payment requirements;

1. The Bidder accepts that GST may require a bank guarantee for any agreed advance payment;

1. The Bidder shall provide warranty and after-sales support in accordance with its offer and the final contract.

Bidder: ______________________________

Company: ____________________________

Authorized Representative: _____________

Position: _____________________________

Date: ________________________________

Signature / Stamp: _____________________
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Instructions to Apply for E-Tender 


 
 


In order to apply for E-Tender, company needs to be registered on procurement web-page www.tenders.ge .  


To start registration process, please press “Sign Up” button on the right side of the site. 


 


E-Tender consists of 5 informational tabs. 
 


§ Description 


§ Questions 


§ Proposal 


§ Discounting (If Enabled) 


§ Results 


§ Clarifications 


 


1. Description 


In the description tab you can find short information about the tender content and requirements. Full tender documentation 


can be downloaded from the attached files at the bottom of the announcement text. 


  


 


On the right side of the page you can view the counter that shows deadline of 


submitting the offer for the current tender.  


 


Additional information shows:  
 


§ Bid submission start time; 


§ Discounting Type: No Discounting, 3 Step Discounting, Reverse/Forward 


Discounting; 


§ Prequalification option; 


§ Bid reduction Step (If discounting is enabled). 


 


 


 


2. Questions 


 
In the following tab companies have possibility to ask questions directly to the procurer representative and receive the 


answer in the system. In order to use the following tab, user needs to be signed in.  Questions asked by the company as well 


as the received answers are visible for all users, however the author of the question is hidden even for the procurer. 


 


 







 


3. Proposal 


 
From proposal tab companies can apply for the tender.  


 


 


 


In order to apply for the tender, user should be signed in. 


In case your company is not registed on our web-page, 


please proceed with “Sign Up” button.  


 


 


 


 


 


After signing in, you will be directed to payment page. 


Applying to e-tender costs 20 Georgian Lari. For making 


payment, press “Process Payment”. In case of 


troubleshooting with the payment, please contact us: 


E-mail: info@tenders.ge 


Tel: +995 595 383635 


  


 


 


 


After Successful payment, you can start uploading the 


tender proposal by pressing “File Upload”. 


 


 


 


 


 


Number of files as well as the file types uploaded in tender 


are not limited. 


In case you want to delete uploaded file, press “Delete”. 
 


After uploading all the required documents, you can 


indicate the bid price and press “Save Price”. 


Please note that after saving the price, you will not be able 


to delete or add files to the proposal documents. 


 


 


 


 


 


 







 


 


After saving the initial price, your bidding documents are 


successfully stored in the system. In case of willing to 


reduce the price before tender deadline, you can indicate 


the new price and press “Update Price”. 


 


Reducing the price should be done in accordance with the 


bid reduction step (In case it is enabled in the tender). 
 


 


 


 


 


4. Results 


 


After the tender submission deadline, participant company can view the following information: Tender participants, 


competitor prices and uploaded documentation. Green background highlights the supplier with the lowest bid. 


 


Please note, that visibility of tender results can be totally or partially restricted by the procurer request: 


§ Tender results can be fully closed only if the tender is announced without auction; 


§ In case any type of auction is available in the tender, suppliers will definitely see the prices of the competitors. 


Therefore the visibility of competitor names and their documentation can be restricted by the procurer.  


 


 


 


 


 


 


 


 


 


 







5. Clarifications 


 


After the tender deadline has passed, clarification tab is enabled. During the evaluation period procurer and supplier can 


communicate using clarifications tab, so all the exchanged files and information are stored in the system.  


 


Clarification statuses: 


§ Received – Clarification request has been received from procurer; 


§ Sent – Supplier has replied to clarification request. 


 


 


 


 


 


 


 


 


 


 


 


 


 


 


 


 


 


By pressing the button “Clear” you can delete the attached files and typed text before sending.  


* Please note that the communication can be initiated only by procurer representative. 


 






image1.jpg




image2.emf
Annex 2 - Technical  Requirements.docx


