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Technical Requirements
1. Dewatered Sludge Containers
Quantity: 2 (two) units;

Application: The containers shall be specifically suitable for the transportation of dewatered wastewater sludge and shall be suitable for outdoor operation under industrial conditions.

Minimum Technical Requirements
	Parameter
	Minimum Requirement

	Quantity
	2 units

	Nominal capacity
	20 m³ each

	Application
	Dewatered sludge transportation

	Construction
	Heavy-duty welded steel construction

	Operation
	Outdoor / industrial operation

	Corrosion protection
	Corrosion-resistant protective coating

	Hooklift compatibility
	Fully compatible with the supplied Hooklift system

	Loading/unloading
	Suitable for safe mechanical loading and unloading

	Structure
	Reinforced heavy-duty construction

	Unloading
	Rear unloading door

	Support
	Rollers/support rollers suitable for Hooklift operation



The Supplier shall state the actual container capacity, dimensions, tare weight and maximum permissible gross weight in its Technical Compliance Table. The container construction shall be suitable for the weight, characteristics and handling requirements of dewatered sludge. The containers shall be designed to withstand repeated loading, transportation, unloading and outdoor operation. The container shall have appropriate structural reinforcement to ensure safe operation under the intended working conditions. The container shall be equipped with a suitable rear door or equivalent unloading arrangement allowing safe and efficient unloading of the dewatered sludge. The containers shall include all rollers, hook bar/interface components, supports and other standard components necessary for operation with the proposed Hooklift system.

2. Hooklift System
Quantity: 1 (one) unit;

Application: The supplied Hooklift system shall be a heavy-duty system designed for industrial and municipal applications and shall be fully compatible with both supplied 20 m³ containers.
The system shall:
· allow safe loading of the containers;
· allow safe unloading of the containers;
· allow secure transportation of the containers;
· be suitable for repeated industrial use;
· be fully compatible with the proposed tractor;
· be fully compatible with the proposed containers;
· be capable of handling the maximum permissible load of the supplied containers;
· comply with applicable European standards and safety requirements.
The Supplier shall provide the complete Hooklift system, including all components required for normal operation. The Hooklift system shall include all hydraulic, mechanical and structural components required for safe and reliable operation. The system shall have appropriate mechanisms for securing the container during transportation. The Bidder shall clearly describe the method of connecting and operating the Hooklift system with the proposed tractor.
3. Tractor
Quantity: 1 (one) unit;

Application: The tractor shall be suitable for transporting and operating the supplied Hooklift system and shall be capable of safely handling the maximum permissible load of the proposed containers. The tractor shall be suitable for industrial operation at the Gardabani Sewage Treatment Plant and associated transportation activities.

Minimum Technical Requirements
	Parameter
	Minimum / Required Specification

	Quantity
	1 unit

	Engine
	Diesel

	Drive
	4×4

	Engine power
	Minimum 130 hp

	Hydraulic system
	Suitable for supplied Hooklift system

	Hydraulic pump
	Minimum 70 l/min or sufficient for the proposed Hooklift system

	PTO
	Suitable for the supplied Hooklift system

	Transmission
	Suitable for heavy-duty operation and transportation

	Lifting capacity
	Minimum 7,800 kg or sufficient for the proposed Hooklift/container combination

	Application
	Heavy-duty industrial operation

	Air conditioning
	Required

	Air compressor
	Required

	Counterweight
	To be provided as required for safe Hooklift operation



The Bidder may offer a tractor with higher technical specifications than the minimum requirements. The proposed tractor shall be technically compatible with the supplied Hooklift system without requiring modifications that are not included in the Bidder’s offer.
4. Compatibility Requirements
1. The Supplier shall ensure full compatibility between: Tractor → Hooklift System → Containers
2. The Bidder shall confirm that the proposed combination constitutes a complete operational system.
3. Any additional equipment, adapters, hydraulic components, fittings, brackets or other components required for
complete operation shall be included in the offered price.
4. No additional payment shall be accepted for components that are necessary for safe and normal operation of the complete system but were omitted from the initial offer.
5. Safety Requirements
1. All supplied equipment shall be new and suitable for the intended industrial application, unless otherwise explicitly agreed by GST. 
2. The equipment shall comply with applicable European technical and safety requirements. 
3. The Hooklift system shall include appropriate mechanical and/or hydraulic safety locking arrangements to prevent unintended movement or release of the container during transportation. 
4. The Supplier shall provide operating and safety instructions in Georgian and/or English.
6. Corrosion Protection and Finish
The containers shall be suitable for outdoor operation and shall have an appropriate corrosion-resistant protective
coating. The Bidder shall describe:
· steel grade/material;
· surface preparation;
· corrosion protection method;
· primer/coating system;
· final coating;
· coating thickness, where applicable.

7. Condition of Goods
Unless otherwise stated in the Bidder’s offer and expressly accepted by GST:
· all equipment shall be new;
· the tractor shall be a new or unused unit;
· the containers shall be newly manufactured;
· the Hooklift system shall be newly manufactured;
· the supplied equipment shall not have been previously used for commercial or industrial operation.
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