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TECHNICAL SPECIFICATIONS
For the supply of truck scales for weighing heavy-duty vehicles up to 100 tons for the RMG "Auramine" production site at the Bektakari Mine




TECHNICAL SPECIFICATIONS
For the supply of truck scales for weighing heavy-duty vehicles up to 100 tons

	№
	Section
	Description of Specifications and Product Requirements

	1
	Product Name
	Electronic truck scale (above-ground, foundation-based), 18 m, capacity up to 100 tons, for weighing cement trucks.

	2
	Compliance with Quality and Safety Requirements
	Product compliance with technical regulations, safety standards, and quality parameters must be confirmed by a certificate of conformity. 
The truck scale must meet regulatory requirements and be registered in the State Register of Measuring Instruments.

	3
	Manufacturing
	The truck scale must be manufactured for the existing concrete foundation on the Customer's premises in accordance with the dimensions provided in the drawing attached to these Technical Specifications.

	4
	Completeness
	1. Set of modules for scale platform assembly.
1. Complete set of hardware/parts for scale installation.
1. Set of load cells, 8 units, rated for 40 tons capacity each.
1. Communication cable.
1. Junction box and cable wiring.
1. Installation diagram.
1. Complete set of documentation in Russian, including the truck scale passport/data sheet with a section for verification marks.

	5
	Product Warranty
	The warranty period for the product shall be no less than 5 years from the date of commissioning of the scale.

	6
	Mandatory Documentation Included with Delivery
	Certificate of Conformity, technical documentation in hard copy and electronic format in Russian/Georgian languages:
1. Operating Manual (indicating technical characteristics) in Russian/Georgian languages;
1. Technical description, including wiring diagrams;
1. Spare parts catalogue;
1. Truck scale passport/data sheet.

	7
	Commissioning Procedure
	Commissioning of the truck scale shall be performed on the Buyer's premises by the Supplier's specialists.

	8
	Supplier Requirements

	Must be a manufacturer of truck scales or an official authorized dealer of a truck scale manufacturer. Must have its own service centre and certified specialists qualified/authorized to perform maintenance on truck scales. 
Availability of a spare parts inventory in stock. Capacity and authorization to conduct training for the Buyer’s staff on the Buyer's premises using certified specialists.

	9
	Supplier Selection Criteria
	Supplier must possess an in-house service centre and certified specialists authorized to maintain the supplied goods throughout the entire operating period. 
Demonstrated operational and supply experience for the offered goods to other enterprises.




Prepared by:
Power Engineer	Bektakari Mine	RMG		 "Auramine" 		Pelisov I.
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