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Technical Terms of Reference

Subject of Tender/Procurement:
Certified industrial equipment for safe inflation of large OTR (Off-The-Road) tires for mining equipment of size 29.5R25. 
Purpose of Equipment:
Ensuring complete safety of personnel during initial inflation and bead seating of tubeless OTR tires on multi-piece rims with lock rings. Eliminating injury risks in case of possible tire burst or ejection of rim locking elements.
Parameters of Serviced Wheels:
· Tire size: from 12.00R20 to 29.5R25 
· Outer tire diameter: up to 1,900 mm 
· Section width: up to 770 mm 
· Assembled wheel weight: up to 850 kg 
· Operating inflation pressure: up to 6.5–9.0 bar 
Mandatory Technical Requirements:
· Certification: Mandatory presence of European CE certificate of conformity, DGUV or OSHA standards. Equipment with a low protection class is not allowed for the tender. 
· [bookmark: _GoBack]Design: Reinforced steel cage (Martins Industries MIC-MINE type or equivalent) or certified hydraulic lock ring restrainer. Internal space must have clearance for 29.5R25 wheel dimensions. 
· Protective Coating: Hot-dip galvanizing or heavy-duty wear-resistant powder coating. 
· Ergonomics: Presence of ramps or a cradle for rolling in the wheel using a loader/OTR tire handler. Design must provide rigid anchoring to the concrete floor foundation.
Automation and Safety Requirements:
· Remote Control: Presence of a remote electronic programmable inflation station (hose/cable length not less than 5 meters from the potential hazard zone). 
· Interlock: Mechanical or pneumatic system preventing air supply when cage doors are open. 
Delivery Terms:
· Accompanying Documentation: Product passport, assembly and operation manual, copy of CE certificate of conformity.
Prepared by: Chief Mechanic						 Melnikov D.A.
