**Technical Data**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Description** | **Quantity** | **Hose connection** | **Diameter Pipe (mm)** | **Photo** |
| Drain Bulldozer unit | 1 | 1"F | 400 - 1500 |  |
| TurboJet rotating chain scraper | 2 | 1"F | 300 |  |
| TurboJet rotating chain scraper 2.4" | 2 | 1"F | 150 - 250 | A yellow and silver toy  AI-generated content may be incorrect. |
| Flex guide for hoses with fix hanger | 4 |   | 170+ | A metal object with many holes  AI-generated content may be incorrect. |
| Pointed nozzle with centre spire | 4 | 1"F | 100-300 |  |
| Pointed nozzle Ø 80 execution long | 4 | 1"F | 150-500 |  |
| BULLDOG 150 mm cage | 4 | 1"F | 170-400 |  |
| 360° Grenade-bomb | 4 | 1"F | 150 - 400 |  |
|  | 25 |  |