****

**Electronic Tender Documentation**

**Procurement of PE 100 (Polyethylene) drinking water Pipes, PE 100 (Polyethylene) for Sewerage Pipes and PE 100 Fittings for drinking water**

**(For identifying supplier for 2025-2026 frame contract)**

***Deadline for submitting bids is 26.09.2025 18:00 (GMT+4) Georgian time***

**1.1 Name of the procurement object**

Georgian Water and Power LTD (ID 203826002) and Gardabani Sewage Treatment Plant LLC (ID 203828313) announce an electronic tender for:

PE 100 (Polyethylene) drinking water Pipes, PE 100 (Polyethylene) for Sewerage Pipes and PE 100 Fittings for drinking water for two years supply.

**1.2. Description of service / work (technical assignment), quantity / volume of the procurement object**

**Technical assignment:**

EN certified PE 100 (Polyethylene) drinking water Pipes, PE 100 (Polyethylene) for Sewerage Pipes and PE 100 Fittings for drinking water, (EN 12201-2 & EN 12201-3) DIN (DIN 4262-1) standard approved by the following entities: DVGW NF114, UKWIR, OVGW, SKZ or some other accredited Western European laboratories. The certificate must be valid.

**Participants must submit the latest version of the EN certificate and the results of the applied research of the laboratory issuing the EN certificate.**

1.In case of winning the tender, the supplier is obliged to send the materials to the laboratory of Western European countries for testing at his own expense within the first three months after signing the contract based on the company request.

**PE Pipes should be tested on following titles:**

* Internal pressure test (ISO 1167) 100 h (4 days)/ 20 °C / 12.0 MPa
* Internal pressure test (ISO 1167) 1000 h (40 days)/ 80 °C / 5.0 MPa
* Melt mass-flow rate MFR (ISO 1133-1)
* Oxidation induction-time OIT (ISO 11357-6)
* Longitudinal reversion (ISO 2505)
* Dimensions
* Assessment of appearance, color

**Fittings (El.Fusion coupler) should be tested on following titles:**

* Melt mass-flow rate MFR (ISO 1133-1)
* Oxidation induction-time OIT (ISO 11357-6)
* Effects of heating (ISO 580)
* Dimensions
* Welding of one fitting at 23 °C by SKZ, subsequent assessment of the weld and cohesion test
* Assessment of the weld and cohesion test on fitting welded by customer

**Fittings for corrugated pipes should be tested on following titles:**

* Tightness of elastomeric sealing ring joints (deformation of pipe and coupler, and angulation)
* Welding of one fitting at 23 °C by SKZ, subsequent assessment of the weld and cohesion test

The results of the laboratory study must be fully shared with company. Samples for testing will be taken randomly by the company. In case of any test results fail or are not satisfied, the supplier must reimburse the damage. The supplier will be penalised. Under this contract, all materials must be replaced, refunds must be made, damages must be compensated, and if the contract is extended, retesting must be performed by the supplier.

All pipes must be marked, in particular with the specifications of the pipe and its length.

Preference will be given to those companies that produce the tendered products (pipes and fittings) in their factory, and if not, then the company participating in the tender must submit the data of the companies producing products compatible with the products required by GWP, who produce similar products.

The supplier is obliged to visit the company (GWP and GST) twice a year and conduct training.

**1.3 Estimation**

The bidder must submit the estimates according to Annex N1 in Excel format. The numbers presented in Annex 1 are approximate quantities of materials purchased for one year and are based on the last 12 months performance .These quantities are not exact and the company does not undertake to purchase this quantity in full within 1 year.

Unit prices must be fixed for at least 6 months. In the event that the supplier increases unit prices, the supplier is obliged to inform the buyer (GWP and GST) about the price change at least 1 month before the price increase and send an appropriate justification, a letter, which will be supported by the factors causing the price increase. The mentioned letter must be accompanied by public links and documentation (invoices, documentation confirming the purchase of raw material, information on changes in energy train prices, etc.). The company reserves the right to request additional documentation in case of need. The company will check the provided information and the market situation. If considering the facts, the price increase will be reasonable, company will agree to the proposal regarding the price increase. In other cases, the supplier has no right to increase the price.

If the company did not find the price change convincing and justified, and also checked and it was found that other companies do not have similar increases, the company has the right not to agree to this price offer. Finally, if no agreement is reached, the terms of termination of the agreement will be considered. Before the termination of the contract, the company must cover the current obligations.

**1.4 Form and place of delivery of goods**

If the supplier can deliver, the delivery locations are as follows:

**City Tbilisi:**

**Warehouse 1**- 12 Feikrebi Street.

**Warehouse 2**- 7 Tskalsadeni Street

**Warehouse 3**- 14 Ivane Iumashevi Street

**Warehouse 4**-Natakhtari

**City Rustavi:**

**Warehouse 5**- Rustavi, 5 Tsminda Nino Street

If the supplier is unable to carry out the transportation, the exact address of the shipment must be indicated.

**1.5 Payment terms**

Payment will be made by consignment, with non-cash payment within 30 (thirty) calendar days (approximate limit up to $ 150,000) after receiving the goods and signing of the relevant acceptance certificate and / or relevant documents. In case of requesting an advance payment, supplier must submit an advance payment guarantee, which must be issued by a bank licensed by Georgia or a bank of a member country of the Organization for Economic Cooperation and Development (OECD).

**1.6 Data to be uploaded / submitted by the bidder in the electronic tender:**

1. Fully filled price table (Annex N1);

2. Extract from the Register of Entrepreneurs and Non-Entrepreneurial (Non-Commercial) Legal Entities, which must be issued after the announcement of this electronic tender;

3. Consent to these tender conditions, for which a signed tender application must be submitted;

4. Information on the materials used Quality certificates issued by the relevant authorities.

**Participants must submit the latest version of the EN certificate and the results of the applied research of the laboratory issuing the EN certificate.**

5. The warranty must apply to the material, companies that offer a 50-year warranty (negotiable) will be given priority during selection.

6.EN certificate (EN 12201-2 & EN 12201-3) DIN (DIN 4262-1) standard approved by the following entities: DVGW  NF114, UKWIR, OVGW, SKZ or some other accredited Western European laboratories

7. The Supplier shall sign the Contractor Management Plan.

8. Offer must be valid for – 90 days

9. By participating in the tender, participants agree to our terms and conditions and the form of the contract that are attached.

10. The company participating in the tender must submit the average financial turnover of the last three years, not less than 5,000,000.00 dollars for the products given in the tender.

11. The company participating in the tender must manufacture large diameter pipes and their corresponding fittings

12. It is preferable the production range of the company producing the products given in the tender must cover the production of water and sewage pipes and fittings together (produced in one factory).

13. The documentation requested by the **Vendor selection and approval - PE Pipes** file must be submitted in full.

14. Filled out **Compliance Questionnaire**

15. The supplier must provide at least 3 references of successful deliveries of PE pipes within the EU in the past 5 years.

16. The company participating in the tender must have its own accredited laboratory.

**Note:**

1. All documents and / or information created by the bidder uploaded in the electronic tender must be signed by an authorized person (if necessary, a power of attorney must be uploaded);
2. All documents and / or information created by the bidder must be confirmed by the electronic signature of the authorized person or the electronic stamp of the company.

**Participation rules:**

**1) Bids must be apploaded on tenders.ge electronic platform, which will be active before the deadline. In case of solid justification, it is possible to receive a proposal by email, but within the tender validity period. Late bids also will not be accepted.**

**2) Deadline for submitting bids is 26.09.2023 18:00 (GMT+4) Georgian time**

**1.7 Signing a contract**

Within the framework of this e-tender, a single contract will be concluded in accordance with the draft contract and the tender proposal attached to this tender.

**1.8 Other requirements**

1.8.1 At the time of submission of the proposal, the bidder should not be:

• in the process of bankruptcy;

• In the process of liquidation;

• In a state of temporary suspension of activities.

1.8.2 Presentation of prices is allowed only in Dollar and Euro

1.8.3 The bid submitted by the bidder must be valid for 90 (ninety) calendar days from the date of receipt of bids.

1.8.4 Georgian Water and Power LTD (ID 203826002) and Gardabani Sewage Treatment Plant LLC (ID 203828313) reserve the right to set the deadline for the tender, change the terms of the tender, notify the tender participants in a timely manner, or terminate the tender at any stage.

The Procurer (Georgian Water and Power Ltd (GWP, ID 203826002)) will identify the winning supplier to the Tender Commission and notify all participating companies of the decision. The Purchaser (Georgian Water and Power Ltd (GWP, ID 203826002)) is not obliged to provide the participating company with a verbal or written explanation of any decision regarding the competition.

The Purchaser (Georgian Water and Power LLC (GWP, ID 203826002)) reserves the right to verify any information received from the Bidders, as well as to obtain information about the Bidder Company or its activities. If it is proved that the information provided by the bidder is not true or falsified, the bidder will be disqualified.

Please note that the Purchaser (Georgian Water and Power Ltd (GWP, ID 203826002) will not receive any oral inquiries for additional information.

***Note: Any other information obtained by other means will not be official and does not give rise to any liability on the part of the Purchaser (Georgian Water and Power LTD (ID 203826002) and Gardabani Sewage Treatment Plant LLC (ID 203828313).***

**1.9 Information for e-tender participants**

1.9.1 Any questions during the tender process must be in writing and the online Q&A mode of tenders.ge portal must be used;

1.9.2 To participate in the electronic tender, the company must be registered on the website [www.tenders.ge](http://www.tenders.ge)

1.9.3 Instructions for participation in the electronic tender on tenders.ge can be found in the attached file

 

**I got acquainted**

/ Signature of the authorized person of the participating company /

**Contact information:**

Procurement representative

Contact person: Magda Lomtatidze

Address: Georgia, Tbilisi, Mtatsminda district, Medea (Mzia) Jugheli street, №10

E-mail Email: [mlomtatidze@gwp.ge](mailto:mlomtatidze@gwp.ge)

Tel: +995 322 931111; 595 22 66 94

Contact person: Mariam Silagadze

Address: Georgia, Tbilisi, Mtatsminda district, Medea (Mzia) Jugheli street, №10

E-mail Email: [msilagadze@gwp.ge](mailto:msilagadze@gwp.ge)

Tel: +995 322 931111 (1147); 599 72 30 03