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Commercial Offer / Price Schedule
The Bidder shall complete the following Commercial Offer:
	№
	Item
	Qty.
	Unit Price EUR
	Total Price EUR

	1
	20 m³ Dewatered Sludge Hooklift Container
	2
	
	

	2
	Hooklift System
	1
	
	

	3
	Tractor suitable for the supplied Hooklift System
	1
	
	

	4
	Standard equipment and accessories
	Included
	
	

	5
	Delivery and transportation to Gardabani -  Wastewater Treatment Plant
	1
	
	

	
	TOTAL PRICE EUR excluding VAT
	
	
	

	
	VAT EUR, if applicable
	
	
	

	
	TOTAL PRICE EUR including VAT
	
	
	



Commercial information to be Provided by the Bidder
	№
	Information
	Bidder’s Offer

	1
	Manufacturer – Containers
	

	2
	Model – Containers
	

	3
	Country of manufacture – Containers
	

	4
	Manufacturer – Hooklift
	

	5
	Model – Hooklift
	

	6
	Country of manufacture – Hooklift
	

	7
	Manufacturer – Tractor
	

	8
	Model – Tractor
	

	9
	Country of manufacture – Tractor
	

	10
	Manufacturing year
	

	11
	Proposed delivery date
	DD/MM/2027

	12
	Delivery location
	Gardabani Wastewater Treatment Plant

	13
	Offer validity period
	

	14
	Payment terms
	___ Days After Delivery

	15
	Advance payment required
	Yes / No

	16
	Advance payment amount
	

	17
	Warranty – Containers
	

	18
	Warranty – Hooklift
	

	19
	Warranty – Tractor
	

	20
	After-sales service location
	

	21
	Service response time
	

	22
	Spare parts availability
	

	23
	Operator training
	Included



Tractor Technical Data
	Parameter
	Bidder’s Offer

	Manufacturer
	

	Model
	

	Country of manufacture
	

	Year of manufacture
	

	Engine power (hp/kW)
	

	Maximum torque (Nm)
	

	Engine displacement
	

	Fuel system
	

	Emission standard
	

	Transmission
	

	Number of forward gears
	

	Number of reverse gears
	

	Wheel formula
	

	Overall length
	

	Overall width
	

	Overall height
	

	Kerb weight
	

	Maximum permissible gross weight
	

	Maximum lifting capacity
	

	Hydraulic pump capacity
	

	Hydraulic operating pressure
	

	Number of hydraulic valves
	

	PTO speeds
	

	Fuel tank capacity
	

	Air conditioning
	Yes/No

	Air compressor
	Yes/No

	Front counterweight
	

	Rear counterweight
	





Hooklift Technical Data
	Parameter
	Bidder to Specify

	Manufacturer
	

	Model
	

	Country of manufacture
	

	Maximum lifting capacity
	

	Maximum container capacity
	

	Suitable container length range
	

	Hook height / hook dimensions
	

	Hydraulic operating pressure
	

	Hydraulic oil flow requirement
	

	Hydraulic cylinder specification
	

	Loading/unloading cycle time
	

	System weight
	

	Required tractor hydraulic capacity
	

	Required PTO characteristics
	

	Safety locking mechanism
	

	Container securing system
	

	Applicable standards
	



Technical Compliance Table
The Bidder shall complete the following table and provide supporting manufacturer documentation where applicable:
	№
	Requirement
	GST Requirement
	Bidder’s Offer
	Comply (Yes/No)
	Supporting Document / Page

	1
	Container quantity
	2 units
	
	
	

	2
	Container capacity
	20 m³ each
	
	
	

	3
	Container application
	Dewatered sludge
	
	
	

	4
	Container construction
	Heavy-duty welded steel
	
	
	

	5
	Corrosion protection
	Required
	
	
	

	6
	Rear unloading door
	Required
	
	
	

	7
	Hooklift compatibility
	Required
	
	
	

	8
	Hooklift system quantity
	1 unit
	
	
	

	9
	Heavy-duty Hooklift
	Required
	
	
	

	10
	Container securing system
	Required
	
	
	

	11
	Tractor quantity
	1 unit
	
	
	

	12
	Engine
	Diesel
	
	
	

	13
	Engine power
	Min. 130 hp
	
	
	

	14
	Drive
	4×4
	
	
	

	15
	Hydraulic capacity
	Min. 70 l/min or sufficient
	
	
	

	16
	Lifting capacity
	Min. 7,800 kg or sufficient
	
	
	

	17
	Air conditioning
	Required
	
	
	

	18
	Air compressor
	Required
	
	
	

	19
	Tractor/Hooklift compatibility
	Required
	
	
	

	20
	Complete system compatibility
	Required
	
	
	

	21
	Operating manuals
	Required
	
	
	

	22
	Spare parts catalogue
	Required
	
	
	

	23
	Warranty
	Min. 12 months
	
	
	

	24
	Delivery
	During 2027
	
	
	

	25
	Exact delivery date
	To be specified
	
	
	



Bidder’s Declaration
The Bidder shall confirm that:
1. The offered equipment complies with the technical requirements specified in this document;
1. The containers, Hooklift system and tractor are fully compatible;
1. The offered system is complete and ready for operation;
1. All necessary standard components are included in the offered price;
1. The proposed equipment is suitable for dewatered sludge transportation;
1. The Bidder has provided accurate technical information;
1. The proposed delivery date falls within calendar year 2027;
1. The Bidder has clearly stated its payment and advance-payment requirements;
1. The Bidder accepts that GST may require a bank guarantee for any agreed advance payment;
1. The Bidder shall provide warranty and after-sales support in accordance with its offer and the final contract.
Bidder: ______________________________
Company: ____________________________
Authorized Representative: _____________
Position: _____________________________
Date: ________________________________
Signature / Stamp: _____________________
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